JOB HAZARD ANALYSIS FORM

**COMPLETE BEFORE BEGINNING WORK**

|  |
| --- |
| **(1) JOB INFORMATION** |
| Date: 8/17/2023 | Job # (If Applicable): | Task Name/Description: Bandsaw  |
| Department: | Supervisor: |
| **(2) JOB/TASK STEPS (Most jobs require 5-10 basic steps)** |
| **Basic Job Step** | **Hazard(s) – (See Sections 3 or EHS Hazard Report)** | **Correct/Safe Work Practice and Hazard Controls/PPE (See Section 4 or EHS Hazard Report)** |
| Perform preoperational check | * None anticipated
 | * Inspect saw, cords, and other equipment per manufacturers guide and do not use if damaged in any way.
* Check to ensure all factory equipped guides/guards are present.
 |
| Adjust the guard and blade | * Cut/puncture/scrape
* Pinch point hazard
 | * Use cut resistant gloves when handling the blade.
* Keep clear of moving parts.
* Pull back long hair.
* Do not remove or alter factory guards.
* Ensure equipment is locked out or unplugged when adjusting.
 |
| Energize equipment and perform cutting operation | * Cut/puncture/scrape
* Pinch point
* Flying debris (eye and body)
* Noise hazard
 | * Wear closed toe shoes when working in any shop environment.
* Use push bar/stick to keep hands away from cutting material.
* Always follow the manufacturer’s operating instructions
* Keep body parts clear of moving machine parts.
* Pull back long hair. Do not wear loose clothing or gloves that can be caught in the bandsaw.
* Wear safety glasses to protect your eyes from flying debris.
* Wear hearing protection if deemed necessary. To determine if hearing protection is required, contact EHS to schedule a noise level test.
* When complete, turn off equipment and wait for blade to stop before removing work items, adjusting equipment, or departing.
 |
| Clean up site  | * Cuts/splinters
* Minor burn hazard
 | * Be aware of sharp edges/splinters on scraps, and do not touch sharp objects.
* Be aware of potentially hot (metal) work material when removing. Material
* Collect/Sweep up all splinters, debris, or other scraps for disposal. Accumulated debris can result in slip hazard or fire hazard.
 |
| **Required Training: - PPE training*** **Equipment specific training (provided by the department)**
* **Hearing conservation training (if deemed necessary)**
* **PPE specific training as necessary**
 | **PPE:** * **Eye protection**
* **Hearing protection (if deemed necessary)**
* **Cut resistant gloves**
* **Closed toe shoes**
 |